**Załącznik nr 2**

**Specyfikacja techniczna szaf teletechnicznych Biura Infrastruktury IT w ORLEN S. A.**

Przedmiotem postępowania jest zakup niezbędnego osprzętu i wyposażenia dla 10 szaf teletechnicznych w celu modernizacji istniejących węzłów teletechnicznych oraz doprowadzeniu ich do aktualnego standardu Biura Infrastruktury IT ORLEN S.A.

Szczegółowa specyfikacja techniczna wyposażenia znajduje się w poniższej tabeli:

|  |  |  |  |
| --- | --- | --- | --- |
|  | Wyposażenie szafy | R&M |  |
|  | **1. Elementy bazowe** |  | **ilość** |
| 1 | R512721 | Panel HD 19" 1U black empty standard | 60 |
| 2 | R512731 | Connection Module Holder HD, 4x 12-port/s, Cat. 6A, black (1-48) | 60 |
| 3 | R510088 | Connection Module Cat. 6A, 1xRJ45/s, Special x100, cena za 1 modul | 2700 |
| 4 | R308247 | Installation Cable Cat. 6A, U/FTP, 4P, 650 MHz, LSZH,grey, Dca, 500 m | 5 |
| 5 | R878004 | Patch Cord CU PATL C6A S RD 0.5m | 400 |
| 6 | R876578 | Patch Cord CU PATL C6A S RD 0.8m | 750 |
| 7 | R878005 | Patch Cord CU PATL C6A S RD 1m | 750 |
| 8 | R878006 | Patch Cord CU PATL C6A S RD 1.5m | 400 |
| 9 | R875788 | Patch Cord CU PATL C6A S RD 2m | 250 |
| 10 | R502280 | Prowadnica patchcordów 90 mm, metal | 65 |
| 11 | R516050 | Wiring Tool-Cat6A-ISO | 2 |
| 12 | R804325 | Cable-Preparation Tool-Cat6A (ISO) | 2 |
| 13 | R380387 | inteliPhy net Pro In-House 1 rack includes 1 year AMC | 100 |